\section{include/conio.h File Reference}
\label{conio_8h}\index{include/conio.h@{include/conio.h}}
Interface: console input / output. 

{\tt \#include $<$config.h$>$}\par
\subsection*{Defines}
\begin{CompactItemize}
\item 
\#define {\bf cls}()\ lcd\_\-clear()
\end{CompactItemize}
\subsection*{Functions}
\begin{CompactItemize}
\item 
void {\bf delay} (unsigned ms)
\begin{CompactList}\small\item\em delay approximately ms m\-Sec \item\end{CompactList}\end{CompactItemize}


\subsection{Detailed Description}
Interface: console input / output. 

\begin{Desc}
\item[Author:]Markus L. Noga $<${\tt markus@noga.de}$>$\end{Desc}
\begin{Desc}
\item[Warning:]If CONF\_\-LCD\_\-REFRESH is set in config.h, the kernel will refresh the display automatically every 100ms. Otherwise, display updates are realized exclusively by {\bf lcd\_\-refresh()}{\rm (p.\,\pageref{sys_2lcd_8h_a16})}.\end{Desc}
\begin{Desc}
\item[Display positions]Digit display positions are denumerated from right to left, starting with 0 for the digit to the right of the running man.\end{Desc}
\begin{Desc}
\item[]LCD Postions: 5 4 3 2 1 \{man\} 0\end{Desc}
\begin{Desc}
\item[]NOTE: Position 5 is only partially present on the LCD display.\end{Desc}
\begin{Desc}
\item[Native segment masks]In these bitmasks, bit 0 toggles the middle segment. Bit 1 toggles the top right segment, and the remaining segments are denumerated counterclockwise. The dot isn't encoded because it is desirable\end{Desc}


Definition in file {\bf conio.h}.

\subsection{Define Documentation}
\index{conio.h@{conio.h}!cls@{cls}}
\index{cls@{cls}!conio.h@{conio.h}}
\subsubsection{\setlength{\rightskip}{0pt plus 5cm}\#define cls()\ lcd\_\-clear()}\label{conio_8h_a0}




Definition at line 233 of file conio.h.

Referenced by Display\-State::disable(), kmain(), main(), show\_\-off(), and show\_\-on().

\subsection{Function Documentation}
\index{conio.h@{conio.h}!delay@{delay}}
\index{delay@{delay}!conio.h@{conio.h}}
\subsubsection{\setlength{\rightskip}{0pt plus 5cm}void delay (unsigned {\em ms})}\label{conio_8h_a1}


delay approximately ms m\-Sec 

\begin{Desc}
\item[Parameters:]
\begin{description}
\item[{\em ms}]approximate time in ms \end{description}
\end{Desc}


Definition at line 204 of file conio.c.

Referenced by kmain(), and show\_\-on().