\section{include/swmux.h File Reference}
\label{swmux_8h}\index{include/swmux.h@{include/swmux.h}}
Interface: direct control of a touch sensor multiplexor. 

{\tt \#include $<$config.h$>$}\par


\subsection{Detailed Description}
Interface: direct control of a touch sensor multiplexor. 

\begin{Desc}
\item[Author:]Mark Falco ({\tt falcom@onebox.com})\end{Desc}
The Touch\-Sensor Multiplexor is a device which allows three Touch\-Sensors to be connected to a single input port.

This code applies to the touch sensor multiplexor (swmux) that can be ordered from {\tt http://www.techno-stuff.com}, tweaking the ranges in {\bf swmux.c}{\rm (p.\,\pageref{swmux_8c})} should make it work with other similar multiplexors

Definition in file {\bf swmux.h}.